For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster System Check? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 |

1. Disconnect the instrument cluster connector.
2. Connect a jumper to connector terminal A1 of the instrument cluster to ground.

Does the CHECK GAUGES indicator illuminate?

--

Go to Step 3

Go to Step 4

3 |

1. Connect the instrument cluster connector.
2. Connect a jumper to connector terminal A13 of the instrument cluster to ground.

Does the CHECK GAUGES indicator illuminate?

--

Go to Step 5

Go to Step 7

4 | Inspect the instrument cluster connector for proper terminal contact. Was a poor connection found? | -- | Go to Step 8 | Go to Step 9
5 | Inspect for an open in CKT 35 (DK GRN). Was there a problem with CKT 35? | -- | Go to Step 10 | Go to Powertrain Control Module Diagnosis
6 | Inspect for an open in CKT 25 (BRN). Was there a problem with CKT 25? | -- | Go to Step 11 | Go to Powertrain Control Module Diagnosis
7 | Inspect the instrument cluster connector for proper terminal contact. Was a poor connection found? | -- | Go to Step 8 | Go to Step 9
8 | Repair the instrument cluster terminal. Refer to Terminal Repair in Wiring Systems. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
9 | Replace the instrument cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges, and Console. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
10 | Repair the open in CKT 35 (DK GRN). Refer to Repairing Damaged Wire Insulation in Wiring Systems. Is the repair complete? | -- | Go to Instrument Cluster System Check | --
11 | Repair the open in CKT 25 (BRN). Refer to Repairing Damaged Wire Insulation in Wiring Systems. Is the repair complete? | -- | Go to Instrument Cluster System Check | --