For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Interior Lights System Check? | -- | Go to Step 2 | Go to Interior Lamps System Check
2 |

1. Disconnect the remote function actuator (RFA) module connector C1.
2. Connect a fused jumper from the remote function actuator (RFA) module connector cavities F1 (LT GRN/BLK) to F16 (BLK).

Do all of the courtesy lamps turn on?

--

Go to Step 3

Go to Step 4

3 | Replace the remote function actuator (RFA) module. Refer to Remote Control Door Lock Receiver Replacement in Keyless Entry. Is the RFA module replacement complete? | -- | Go to Interior Lamps System Check | --
4 | Inspect CKT 394 (LT GRN/BLK) for an open. Refer to Testing for Continuity in Wiring Systems. Was an open found? | -- | Go to Step 5 | Go to Step 6
5 | Repair the open in CKT 394 (LT GRN/BLK). Refer to Wiring Repairs in Wiring Systems. Is the circuit repair complete? | -- | Go to Interior Lamps System Check | --
6 | Inspect CKT 1250 (BLK) for an open. Refer to Testing for Continuity in Wiring Systems. Was an open found? | -- | Go to Step 7 | Go to Step 8
7 | Repair the open in CKT 1250 (BLK). Refer to Wiring Repairs in Wiring Systems. Is the circuit repair complete? | -- | Go to Interior Lamps System Check | --
8 | Replace the body control module (MALL). Refer to Body Control Module Replacement in Body Control Systems. Is the MALL module replacement complete? | -- | Go to Interior Lamps System Check | --