For 1990-2009 cars

### Assembly Procedure

#### Tools Required

• | J 41352 Modular Column Holding Fixture

• | J 23653-SIR Lock Plate Compressor

Important: The column must be in the 12 o'clock position.

1. Align the steering column to the 12 o'clock position.
2. Install the wave washer.
3. Install the hanging SIR coil assembly onto the race and upper shaft assembly.
4. Center the SIR coil assembly. Refer to Inflatable Restraint Coil Centering - Off Vehicle (Column Shift And Floor Shift) .
5. The new SIR coil assembly will come precentered. Once installed, pull the tab and remove.
6. If the SIR coil assembly is completely off refer to the upper tilt head component assembly Turn Signal Cancel Cam and Upper Bearing Inner Race - Assemble - Off Vehicle .
7. Install the wire protector into the support bracket.
8. Install the retaining ring.
9. Install the SIR coil assembly connector (1) to the fused jumper assembly connector (2).
10. Put the wire harness assembly into the wire harness strap (1) using toolJ 41352 .