For 1990-2009 cars

## Evaporative Emission Canister Purge Solenoid Valve Replacement VIN K

### Removal Procedure

1. Disconnect the electrical connector and hoses from the EVAP purge solenoid.
2. Bend the tab on the solenoid mounting bracket to remove the EVAP purge solenoid.
3. Remove the EVAP purge solenoid.

### Installation Procedure

1. Bend the tab on the EVAP purge solenoid mounting bracket to install the EVAP purge solenoid.
2. Install the EVAP purge solenoid.
3. Connect the hoses and the electrical connector to the solenoid.

## Evaporative Emission Canister Purge Solenoid Valve Replacement VIN 1

### Removal Procedure

1. Disconnect the electrical connector and hoses from the EVAP purge solenoid.
2. Bend the tab on the solenoid mounting bracket to remove the EVAP purge solenoid.
3. Remove the EVAP purge solenoid from the bracket.

### Installation Procedure

1. Bend the tab on the EVAP purge solenoid mounting bracket to install the solenoid.
2. Install the EVAP purge solenoid.
3. Connect the hoses and the electrical connector to the EVAP purge solenoid.