For 1990-2009 cars

### Removal Procedure

1. Remove the door lock switch bezel (1). Refer to Front Side Door Trim Panel Insert Replacement or Rear Side Door Trim Panel Insert Replacement .
2. Release the lock rod knob retainers.

Use a small, flat-bladed tool.

3. Remove the lock rod knob.

### Installation Procedure

1. Align the lock rod knob with the door lock switch bezel (1).
2. Install the lock rod knob to the bezel.

Push downward on the knob.

3. Install the door lock switch bezel. Refer to Front Side Door Trim Panel Insert Replacement or Rear Side Door Trim Panel Insert Replacement .