For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the bolts (3) that retain the park/turn signal lamp (2) to the impact bar (1).
3. Remove the electrical bulb/socket from the park/turn signal lamp (2).
4. Remove the park/turn signal lamp (2).

### Installation Procedure

1. Install the electrical bulb/socket into the park/turn signal lamp (2).
2. Install the park/turn signal lamp (2).
3. Install the bolts (3) in order to retain the park/turn signal lamp (2) to the impact bar (1).
4. Lower the vehicle.