For 1990-2009 cars

### Removal Procedure

1. Pull the ashtray up and out in order to remove the ashtray.
2. Use the following procedures in order to remove the bulb cover:

2.1. | Squeeze the tangs on each side of the bulb cover.

2.2. | Pull the bulb cover sideways in order to release the bulb cover.

2.3. | Twist and pull the bulb cover.

3. Pull outward in order to remove the bulb.

### Installation Procedure

1. Install the bulb by pushing the bulb into the socket.
2. Twist and push the bulb cover in order to install the bulb cover.
3. Squeeze the tangs on each side of the bulb cover.
4. Push the bulb cover in order secure the bulb cover.
5. Install the ashtray by pushing the ashtray inward and downward.