For 1990-2009 cars

Name | Hydra-matic 4T65-E
--- | ---
RPO Codes | M15/MN3/MN7
Production Location | Warren, MI
Vehicle Platform (Engine/Transmission) Usage | H
Transaxle Drive | Transverse Mounted Front Wheel Drive
1st Gear Ratio | 2.921:1
2nd Gear Ratio | 1.568:1
3rd Gear Ratio | 1.000:1
4th Gear Ratio | 0.705:1
Reverse | 2.385:1
Torque Converter Size (Diameter of Torque Converter Turbine) | 245 mm (M15) 258 mm (MN3/MN7)
Pressure Taps | Line Pressure
Transaxle Fluid Type | Dexron™ III
Transaxle Fluid Capacity (Approximate) | Bottom Pan Removal: 7.0 L (7.4 qts) Complete Overhaul: 9.5 L (10.0 qts) Dry: 12.7 L (13.4 qts)
Transaxle Type: 4 | Four Forward Gears
Transaxle Type: T | Transverse Mount
Transaxle Type: 65 | Product Series
Transaxle Type: E | Electronic Controls
Chain Ratios (Designates Number of Teeth on the Drive/Driven Sprockets) | 35/35 37/33
Final Drive Ratios | 2.86, 3.05, 3.29
Overall Final Drive Ratios | 2.86, 3.05, 2.93
Position Quadrant | P, R, N, D, 3, 2, 1 or P, R, N, OD, 2, 1
Case Material | Die Cast Aluminum
Transaxle Weight Dry | 87.9 kg (194.2 lbs)
Transaxle Weight Wet | 97.0 kg (214.4 lbs)
Maximum Trailer Towing Capacity | 907 kg (2000 lbs)
Maximum Gross Vehicle Weight (GVW) | 2903 kg (6,400 lbs)