For 1990-2009 cars

#### Tools Required

J 21854-01 Pivot Pin Remover

1. Remove the steering column pass key lock cylinder set. Refer to Steering Column Lock Cylinder Set - Disassemble - Off Vehicle
2. Remove the column housing cover end cap (1).
3. Remove the 3 pan head 6-lobed socket tapping screws. (1) at 12 o'clock, (2) at 3 o'clock and (3) at 8 o'clock.
5. Remove the lock housing cover assembly (1).
6. Remove the column housing cover end base plate (2) and the dimmer switch rod actuator (3).
7. Remove the pivot and pulse switch assembly only. Refer to Windshield Wiper and Washer Switch Assembly - Disassemble - Off Vehicle
8. Remove the tilt spring assembly only. Refer to Tilt Spring - Disassemble - Off Vehicle
9. Remove the 2 pivot pins (1) using tool J 21854-01
10. Reinstall the tilt lever (2).
11. Pull back on the tilt lever (2) and pull steering column housing assembly (1) down and away from column.
12. Remove the tilt lever (2).