For 1990-2009 cars

### Removal Procedure

1. Pull the ashtray upward and outward in order to remove the ashtray.
2. Squeeze the tangs on each side of the bulb cover in order to remove the bulb cover.

Pull the bulb sideways in order to release the bulb.

3. Twist and pull the bulb cover in order to remove the bulb cover.
4. Pull outward on the bulb in order to remove the bulb.

### Installation Procedure

1. Push the bulb into the socket.
2. Squeeze the tangs on both side of the bulb cover in order to install the cover.

Push the cover in order to secure the cover.

3. Push inward and downward on the ashtray in order to install the ashtray.