For 1990-2009 cars

#### Electronic Suspension Control (CCR) Module

Connector Part Information |

• | 12045537

• | 32 Way F Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C1 | - | - | Not Used
C2 | DK BLU | 1308 | CCR Module Lateral Acceleration Signal Output
C3 | PPL/WHT | 1490 | CCR Module Signal - WOT
C4 | - | - | Not Used
C5 | LT GRN | 1435 | CCR Switch Signal (Normal)
C6 | BRN/WHT | 1434 | CCR Signal Switch (Firm)
C7 | DK GRN/WHT | 817 | Vehicle Speed Signal
C8 | - | - | Not Used
C9 | DK GRN | 1437 | CCR LED Feed (Firm)
C10 | PNK | 1438 | CCR LED Feed (Normal)
C11- C12 | - | - | Not Used
C13 | WHT/BLK | 1006 | RH Front Ride Control Strut Motor Feed (Increase)
C14 | YEL | 1014 | RH Rear Ride Control Strut Motor Feed (Increase)
C15 | LT BLU | 1770 | Ride Control Diagnostic Signal
C16 | BRN | 641 | Fused Output (Ign)
D1 | BLK/WHT | 251 | Ground
D2 | LT GRN | 1826 | Ride Control Diagnostic Enable Signal
D3 | DK GRN/WHT | 1016 | RH Rear CCR Strut Position Signal
D4 | BRN/WHT | 1012 | LH Rear CCR Strut Position Signal
D5 | LT BLU | 1008 | RH Front CCR Strut Position Signal
D6 | BRN/WHT | 1004 | LH Front CCR Strut Position Signal
D7 | GRY | 1309 | CCR Module Lateral Acceleration Signal Input
D8 | BRN | 1009 | RH Front Ride Control Strut Motor Feed (Decrease)
D9 | PPL | 1017 | RH Rear Ride Control Strut Motor Feed (Decrease)
D10 | LT GRN | 1005 | LH Front Ride Control Strut Motor Feed (Decrease)
D11 | RED/BLK | 1013 | LH Rear Ride Control Strut Motor Feed (Decrease)
D12 | - | - | Not Used
D13 | RED | 1448 | LH Front Ride Control Strut Motor Feed (Increase)
D14 | RED | 1010 | LH Rear Ride Control Strut Motor Feed (Increase)
D15 | - | - | Not Used
D16 | BLK/WHT | 251 | Ground