For 1990-2009 cars

#### fluid ind and chime inop

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire Brake Warning System Check performed? | -- | Go to step 2 | Go to Brake Warning System Check
2 |

1. Disconnect the brake fluid level switch.
2. Connect a test lamp between the brake fluid level switch harness connector terminal A and battery positive voltage.

Is the test lamp lit?

--

Go to step 4

Go to step 3

3 | Repair open in circuit 1250 (BLK). Is the repair complete? | -- | Go to Brake Warning System Check | --
4 | Replace the brake fluid level switch. Is the repair complete? | -- | Go to Brake Warning System Check | --