For 1990-2009 cars

1. Remove the indicated control valve body bolts (375-380).
2. Remove the control valve body assembly (300).
3. Remove the six ball check valves (372, 373) from the top of the spacer plate (370).
4. Remove the spacer plate (370), remove the gaskets (369, 371), and remove the screens (374).
5. Remove the case cover pin (410).
6. Remove the four ball check valves (372) from the case cover.