For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)
--- | --- | --- | ---
1 |

1. Move the left front power door lock switch to the LOCK position.
2. Move the left front power door lock switch to the UNLOCK position.
3. Move the right front power door lock switch to the LOCK position.
4. Move the right front power door lock switch to the UNLOCK position.

• | All of the doors lock and stay locked when a lock switch is pressed.

• | All of the doors unlock and stay unlocked when an unlock switch is pressed.

• | Automatic Door Locks Inoperative, Power Locks Operate

• | Power Door Locks Inoperative - All Doors and Switches

• | Power Door Locks Inoperative - All Doors and Switches

• | Power Door Locks Switch Inoperative - One

• | Power Door Locks Inoperative

• | Power Door Locks Inoperative, RKE Operates

• | Power Door Locks Inoperative, RKE Operates

• | Power Door Locks Inoperative - One Motor

• | Power Door Locks Inoperative with Door and Key Switches

• | Power Door Locks Switch Lock Function Inoperative - One

• | Power Door Locks Switch Unlock Function Inoperative - One

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.