For 1990-2009 cars

Remove the fuse block cover (1) in order to access the fuses. Several fuses are also located in the relay center. Perform the following steps in order to remove the fuse block cover:

#### Removal Procedure

1. Depress the release tab.
2. Pull down on the cover (3).

### Installation Procedure

1. Insert tabs on the fuse block cover (3) into the sound insulator.
2. Push upward to fasten the fuse block cover.