For 1990-2009 cars

#### Tools Required

• | J 21465-13 Drive Handle Extension

• | J 36995 Balance Shaft Bearing Remover/Installer

1. Dip the balance shaft bushing in clean engine oil.

Important: The J 36995 installs the balance shaft bushing to the correct depth. The balance shaft bushing is properly installed when J 36995 fully contacts the balance shaft bore or the engine block/transaxle mounting flange.

2. Use the balance shaft bushing installers to install the balance shaft bushing.
3. Remove J 36995 .
4. Dip the balance shaft bearing into clean engine oil.
5. Use J 21465-13 and J 36995 to install the balance shaft bearing into the engine block.