For 1990-2009 cars

### Removal Procedure

Caution: When working with any type of glass or sheet metal with exposed or rough edges, wear approved safety glasses and gloves in order to reduce the chance of personal injury.

1. Remove the trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Door Water Deflector Replacement .
3. Remove the inner and the outer sealing strips.
4. Remove the sash fasteners (3).
5. Remove the window (1) from the outboard side.

### Installation Procedure

Caution: When working with any type of glass or sheet metal with exposed or rough edges, wear approved safety glasses and gloves in order to reduce the chance of personal injury.

1. Install the window from the outboard side (1).
2. Install the sash fasteners (3).
3. Install the inner and the outer sealing strips.
4. Adjust the window. Refer to Front Side Door Window Adjustment .
5. Install the water deflector. Refer to Door Water Deflector Replacement .
6. Install the trim panel. Refer to Front Side Door Trim Panel Replacement .