For 1990-2009 cars

## Outside Mirrors System Check Without A43

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Put the mirror select switch in the left position.
2. Move the power mirror switch up and down.

The left outside power mirror moves smoothly upward and downward.

• | Power Mirrors Inoperative

• | Power Mirrors Inoperative in Up/Down Direction - One

2 | Move the power mirror switch left and right. | The left outside power mirror moves smoothly left and right. | Power Mirrors Inoperative in Left/Right Direction - One
3 |

1. Put the mirror select switch in the right position.
2. Move the power mirror switch up and down.

The right outside power mirror moves smoothly upward and downward.

Power Mirrors Inoperative in Up/Down Direction - One

4 | Move the power mirror switch left and right. | The right outside power mirror moves smoothly left and right. | Power Mirrors Inoperative in Left/Right Direction - One
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.

## Outside Mirrors System Check With A43

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Set the mirror select to LH.
2. Briefly press each of the following mirror switches:

• | LEFT

• | RIGHT

• | UP

• | DOWN

The left mirror moves in the selected direction.

• | Power Mirrors Inoperative

• | Door Functions Inoperative

• | Power Mirrors Inoperative in Left/Right Direction - One

• | Power Mirrors Inoperative in Up/Down Direction - One

2 |

1. Set the mirror select to RH.
2. Briefly press each of the following mirror switches:

• | LEFT

• | RIGHT

• | UP

• | DOWN

The right mirror moves in the selected direction.

• | Power Mirrors Inoperative

• | Power Mirrors Inoperative in Left/Right Direction - One

• | Power Mirrors Inoperative in Up/Down Direction - One

3 | Momentarily press the DRIVER-1 switch. |

• | The following components move to the DRIVER-1 programmed settings:

• | Seat

• | Both outside power mirrors

• | A single beep is heard.

• | Power Mirrors - Memory Functions Inoperative

• | Power Mirrors - Memory Inoperative in One Direction

4 | Momentarily press the DRIVER-2 switch. |

• | The following components move to the DRIVER-2 programmed settings:

• | Seat

• | Both outside power mirrors

• | A single beep is heard.

• | Power Mirrors - Memory Functions Inoperative

• | Power Mirrors - Memory Inoperative in One Direction

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.