For 1990-2009 cars

### Removal Procedure

1. Lower the window.
2. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Starting at one end of the door window inner belt molding pull upward in order to release the molding.

### Installation Procedure

1. Position the door window belt molding over the flange of the door inner panel.
2. Position the notch in the belt molding to the rear stationary window frame.
3. Press down in order engage the door window inner belt molding the entire length, being careful not to distort the belt molding.
4. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .