For 1990-2009 cars

## Filler Panel Replacement - Upper 88/LSS

### Removal Procedure

1. Remove the push-in retainers (2) from the filler panel (1).
2. Remove the upper filler panel (1).

### Installation Procedure

1. Install the upper filler panel (1).
2. Install the push-in retainers (2) .

## Filler Panel Replacement - Upper Regency

### Removal Procedure

1. Remove the push-in retainers (2) from the filler panel (1).
2. Remove the upper filler panel (1).

### Installation Procedure

1. Install the upper filler panel (1).
2. Install the push-in retainers (2) .