For 1990-2009 cars

### Removal Procedure

1. Remove the IP cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement
2. Remove the screws (2).
3. Remove the HUD switch (1) from the IP.
4. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the HUD switch (1) to the IP.
3. Install the screws (2) to the IP.
4. Install the IP cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement .