For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Instrument Cluster System Check? | -- | Go to Step 2 | Go to Instrument Cluster System Check
2 |

1. Disconnect the rear compartment lid latch switch connector.
2. Connect a fused jumper between switch connector terminal B and ground.

Does the TRUNK AJAR indicator illuminate?

--

Go to Step 3

Go to Step 4

3 | Connect a fused jumper between switch connector terminal B and terminal C. Does the TRUNK AJAR indicator illuminate? | -- | Go to Step 5 | Go to Step 6
4 | Inspect for an open in CKT 744 (RED/BLK). Is the wiring OK? | -- | Go to Step 11 | Go to Step 10
5 | Inspect the rear compartment lid latch switch connector for proper terminal contact. Is the terminal contact OK? | -- | Go to Step 8 | Go to Step 7
6 | Inspect for an open in CKT 1350 (BLK/WHT). Is the wiring OK? | -- | Go to Instrument Cluster System Check | Go to Step 9
7 | Repair the poor terminal contact. Did you complete the repair? | -- | Go to Instrument Cluster System Check | --
8 | Replace the rear compartment lid latch switch. Did you complete the repair? | -- | Go to Instrument Cluster System Check | --
9 | Repair the open CKT 1350 (BLK/WHT). Did you complete the repair? | -- | Go to Instrument Cluster System Check | --
10 | Repair the open in CKT 744 (RED/BLK). Did you complete the repair? | -- | Go to Instrument Cluster System Check | --
11 |

1. Inspect the instrument cluster connector C1, terminal B3.
2. Inspect terminal L6 of connector C200 for proper terminal contact.

Are the connector terminal contacts OK?

--

Go to Step 12

Go to Step 7

12 | Replace the instrument cluster. Did you complete the repair? | -- | Go to Instrument Cluster System Check | --