For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to ACCY or RUN.
2. Hold the washer switch in the ON position for less than 1 second.

• | The washer sprays the windshield and continues to spray for 2½ seconds after the switch is released.

• | The wipers run at low speed and continue to run for approximately 6 seconds after the washer cycle is complete, then return to the park position.

• | Washers Inoperative .

• | Wipers Low Mode Inoperative, High Mode Operates .

2 |

1. Turn the wiper switch to DELAY (pulse mode).
2. Activate the delay time by turning the wiper switch.

• | The wipers make one complete sweep, then pause for 0-25 seconds before making the next sweep.

• | The pause time is adjusted by turning the wiper switch through the delay range.

Wipers Delay Mode Inoperative .

3 |

1. Turn the wiper switch to DELAY.
2. Hold the washer switch ON for 1-2 seconds.

• | The washer sprays as long as the washer switch is held ON. The wipers run at low speed during the spray period and continue for 2-4 sweeps after the washer switch is released.

• | The wipers then return to pulse operation.

• | Wipers Delay Mode Inoperative .

• | Washers Inoperative .

4 | Turn the wiper switch to LO. | The wipers run continuously at low speed. |

• | Wipers Low Mode Inoperative, High Mode Operates .

• | Wipers All Modes Inoperative .

• | Wipers Low or High Modes Intermittent .

5 | Turn the wiper switch to HI. | The wipers run continuously at high speed. |

• | Wipers High Mode Inoperative, Low Mode Operates .

• | Wipers All Modes Inoperative .

• | Wipers Low or High Modes Intermittent .

6 | Turn the wiper switch to OFF. | The wipers return to the park position at low speed. |

• | Wipers Blades Do Not Park .

• | Wipers Always On .

7 | Turn the wiper switch to MIST, then release. | The wipers make one complete sweep, then return to the park position. | Wipers High Mode Inoperative, Low Mode Operates .