For 1990-2009 cars

#### Component Resistance Chart

Cavities | Component | Resistance at 20°C (68°F) | Resistance at 88°C (190°F)
--- | --- | --- | ---
A-E | 1-2, 3-4 Shift Solenoid Valve | 19-24 ohms | 24-31 ohms
B-E | 2-3 Shift Solenoid Valve | 19-24 ohms | 24-31 ohms
T-E | Torque Converter Clutch Pulse Width Modulation Solenoid Valve | 10-12 ohms | 13-15 ohms
C-D | Pressure Control Solenoid Valve | 3-5 ohms | 5-6 ohms
S-V | Automatic Transmission Input Speed Sensor | 893-1127 ohms | 1132-1428 ohms
M-L | Automatic Transmission Fluid Temperature Sensor | 3164-3867 ohms | 225-285 ohms