For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Inside Rearview Mirror | Center of the passenger compartment, attached to the windshield | -- | --
IP Fuse Block | Under the left side of the IP, on the left IP sound insulator | Power and Grounding Component Views in Wiring Systems | Electrical Center Identification Views in Wiring Systems
LH Outside Power Mirror | Left hand of the vehicle, on the out side of the left hand front door | -- | --
Park/Neutral Position (PNP) Switch | On the left side of the transaxle, below the exhaust gas recirculation valve | Engine Controls Component Views in Engine | Engine Controls Connector End Views in Engine
C205 (8 cavities) | The body harness to the headliner harness, in the left front of the passenger compartment, on the top of the front pillar | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G105 | In the right front of the engine compartment | Power and Grounding Component Views in Wiring Systems | --
G202 | In the left front of the passenger compartment, behind the left kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
P101 | In the right rear of the engine compartment, near the right front strut tower | Harness Routing Views in Wiring Systems | --
P500 | On the front of the left front door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
S208 | In the body harness, approximately 6 cm (2.4 in) from the center IP harness channel breakout | Harness Routing Views in Wiring Systems | --
S225 | In the body harness, approximately 49.5 cm (19.5 in) from the top edge of the left kick wall channel | Harness Routing Views in Wiring Systems | --
S270 | In the body harness, approximately 8 cm (3.1 in) from the edge of the right IP harness channel end | Harness Routing Views in Wiring Systems | --
S280 | In the body harness, approximately 31.5 cm (12.4 in) from P100 | Harness Routing Views in Wiring Systems | --
S293 | In the body harness, approximately 4 cm (1.6 in) from the instrument cluster breakout | Harness Routing Views in Wiring Systems | --
S332 | In the headliner harness, approximately 23.5 cm (9.3 in) from the automatic day-night mirror breakout | -- | --
S414 | In the body harness, approximately 144 cm (56.7 in) from P408 | Harness Routing Views in Wiring Systems | --