For 1990-2009 cars

### Removal Procedure

1. Pull the trim panel (2) straight away from the vehicle at the following positions:

• | The middle

• | The bottom

2. Pull the trim panel down at the top.
3. Slide the shoulder belt through the slit at the top of the trim panel.
4. Remove the trim panel from the vehicle at the following positions:

• | The top

• | The middle

• | The bottom

### Installation Procedure

1. Slide the shoulder belt through the slit at the top of the trim panel (2).
2. Slide the trim panel into the retainers at the top of the vehicle.
3. Push the trim panel into place.