For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel. Refer to Instrument Panel Assembly Removal in Instrument Panel, Gauges and Console.
2. Remove the fastener from the rear edge of the module.
3. Remove the PASS-Key® II module from the bracket (1).
4. Disconnect the electrical connection(s).

### Installation Procedure

1. Connect the electrical connection(s).
2. Install the PASS-Key® II module to the bracket (1).
3. Install the fastener.
4. Install the instrument panel. Refer to Instrument Panel Assembly Removal in Instrument Panel, Gauges and Console.