For 1990-2009 cars

## Front Upper Speaker Replacement Oldsmobile

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.
2. Place the door trim panel on a clean protected surface.
3. Disconnect the electrical connector.
4. Remove the fasteners (1) retaining the speaker to the door trim panel.
5. Remove the speaker.

### Installation Procedure

1. Align the speaker to the door trim panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the speaker fasteners (1).

Tighten
Tighten the fasteners to 1.4 N·m (12 lb in).

3. Connect the electrical connector.
4. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.