For 1990-2009 cars

1. Use a flat blade screwdriver in order to remove the retaining ring (627) from the second clutch housing.
2. Remove the second clutch backing plate (626). Remove the alternating second clutch fiber plates (624). Remove the second clutch steel plates (625).
3. Remove the second clutch apply plate (716). Remove the second clutch waved plate (623).
4. Use a flat blade screwdriver in order to remove the retaining ring (622) from the second clutch housing.
5. Remove the second clutch spring assembly (621).
6. Remove the second clutch piston assembly (620).