For 1990-2009 cars

### Removal Procedure

1. Partially remove the knee bolster. Refer to Instrument Panel Knee Bolster .
2. Disconnect the electrical connector from the interior lighting control module.
3. Complete the removal of the knee bolster.
4. Remove the interior lighting control module from the knee bolster.

### Installation Procedure

1. Install the interior lighting control module to the knee bolster.
2. Partially install the knee bolster.
3. Connect the electrical connector to the module.
4. Install the knee bolster. Refer to Instrument Panel Knee Bolster .