For 1990-2009 cars

## Sunroof Switch Replacement Buick

### Removal Procedure

1. Using a flat-bladed tool, gently pry the front courtesy / reading lamp tabs inward.
2. Disconnect the electrical connectors.
3. Remove the overhead console.
4. Remove the fasteners (1) securing the power sunroof switch to the overhead console.
5. Remove the power sunroof switch.

### Installation Procedure

1. Install the power sunroof switch into the overhead console.
2. Install the fasteners (1) to secure the power sunroof switch.
3. Connect the electrical connectors.
4. Install the overhead console into the headliner opening.

## Sunroof Switch Replacement Pontiac With CF5

### Removal Procedure

1. Using a flat-bladed tool (1), gently pry the sunroof switch (2) from the headliner.
2. Disconnect the electrical connector.
3. Remove the sunroof switch (2).

### Installation Procedure

1. Connect the electrical connector to the sunroof switch (2).
2. Gently press the sunroof switch (2) into the headliner assembly.

The locking tabs on the switch secure the switch to the headliner assembly.