For 1990-2009 cars

### Removal Procedure

1. Open the door either front or rear.
2. Peel the weatherstrip from the flange.
3. Remove the screws from the auxiliary (dogleg) weatherstrip (rear door only).
4. Remove the auxiliary weatherstrip.

### Installation Procedure

1. Align the weatherstrip to the door and press the weatherstrip to the flange in all directions.
2. Install the auxiliary weatherstrip (rear door only).
3. Install the screws to the rear door auxiliary weatherstrip in order to secure.
4. Close the doors.