For 1990-2009 cars

### Removal Procedure

1. Fold the trim assembly (1) until the bottom edges meet in the center, as shown in the illustration.
2. Lift and remove the trim (1) from the rear compartment.

### Installation Procedure

1. Install the still-folded trim (1) into the rear compartment.
2. Smooth the trim out in order to fit the rear compartment in the following sequence:

2.1. | Contour at the rear end of the panel

2.2. | Contour at the quarter panel

2.3. | Contour at the front of the panel