For 1990-2009 cars

## Control Assembly Replacement - Passenger Buick

### Removal Procedure

1. Remove the door handle insert. Refer to Front Side Door Trim Panel Insert Replacement in Doors.
2. Remove the right door pad. Refer to Front Side Door Trim Panel Replacement in Doors.
3. Remove the 2 retaining screws.
4. Remove the passenger climate control.

### Installation Procedure

1. Install the passenger climate control.
2. Install the 2 retaining screws.
3. Install the right door pad. Refer to Front Side Door Trim Panel Replacement in Doors.
4. Install the door handle insert. Refer to Front Side Door Trim Panel Insert Replacement in Doors.

## Control Assembly Replacement - Passenger Oldsmobile

### Removal Procedure

1. Remove the door handle insert. Refer to Front Side Door Trim Panel Insert Replacement in Doors.
2. Remove the passenger climate control/power window switch plate.
3. Disconnect the electrical connector.
4. Remove the passenger climate control from the switch plate.

### Installation Procedure

1. Install the passenger climate control to the switch plate.
2. Connect the electrical connector.
3. Install the switch plate to the armrest.
4. Install the door handle insert. Refer to Front Side Door Trim Panel Insert Replacement in Doors.