For 1990-2009 cars

## Rear Bumper Fascia Molding Replacement Buick

### Removal Procedure

1. Gently peel the following components away from the fascia (1):

• | The molding (2)

• | The nameplate (3)

2. Clean the attaching surface with a general adhesive remover.

### Installation Procedure

1. Peel the backing away from the adhesive on the new molding (2) and on the nameplate (3).
2. Apply the following components to the fascia (1):

• | The molding (2)

• | The nameplate (3)

## Rear Bumper Fascia Molding Replacement Oldsmobile Regency

### Removal Procedure

1. Gently peel the molding (2) away from the fascia (1).
2. Clean the attaching surface with a general adhesive remover.

### Installation Procedure

1. Peel the backing away from the adhesive on the new molding (2).
2. Apply the molding onto the fascia (1).

## Rear Bumper Fascia Molding Replacement Oldsmobile 88

### Removal Procedure

1. Gently peel the molding (2) away from the fascia (1).
2. Clean the attaching surface with a general adhesive remover.

### Installation Procedure

1. Peel the backing away from the adhesive on the new molding (2).
2. Apply the molding onto the fascia (1).