For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Exhaust Pipe to the Front Stabilizer Bar | 37 mm | 1.45 in
Heatshield to the Converter | 31 mm | 1.22 in
Intermediate Pipe/Resonator and the Splash Shield to the Fuel Tank facing the RH of the vehicle | 37 mm | 1.45 in
Intermediate Pipe/Resonator and the Splash Shield at 55 degrees to the heat shield toward facing to the rear of the vehicle | 48 mm | 1.89 in
Intermediate Pipe/Resonator and the Splash Shield at 80 degrees to the heat shield toward facing to the rear of the vehicle | 24 mm | 0.94 in
Intermediate Pipe/Resonator and the Splash Shield at 225 degrees to the heat shield facing to the front of the vehicle | 43 mm | 1.69 in
Intermediate Pipe/Resonator and the Splash Shield at 165 degrees to the heat shield facing to the front of the vehicle | 29 mm | 1.14 in
Intermediate Pipe/Resonator and the Splash Shield at 45 degrees to RH of the of the Rear Stabilizer Bar | 23 mm | 0.90 in
Tailpipe to the Muffler | 13 mm | 0.5 in
Tailpipe to the Rear Fascia (Pontiac) | 49 mm | 1.9 in
Tailpipe to the Rear Fascia (Oldsmobile Eighty-Eight) | 24 mm | 0.94 in
Tailpipe to the Rear Fascia (Buick LeSabre) | 29 mm | 1.14 in