For 1990-2009 cars

#### Tools Required

J 23653-SIR Lock Plate Compressor

1. Install the inner race (2). Lubricate with synthetic grease.
2. Install the upper bearing inner race seat (1).
3. Install the upper bearing spring (3).
4. Install the turn signal cancel cam assembly (2). Lubricate with synthetic grease.
5. Install the shaft lock (1).
6. Install the new bearing retainer (1) using J 23653-SIR
7. Install the SIR coil assembly. Refer to Inflatable Restraint Steering Wheel Module Coil Assemble - Off Vehicle