For 1990-2009 cars

Table 1: | Pass-Key® II Theft Deterrent Module
Table 2: | Rear Compartment Lid Tamper Switch

#### Pass-Key® II Theft Deterrent Module

Connector Part Information |

• | 12110259

• | 16-Way F Micro - Pack 100 Series (GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | RED | 1642 | Fused Output - Battery
A2 | PNK | 139 | Fused Output - IGN
A3 | DK BLU | 229 | Vehicle Anti-Theft System Signal - Disable Engine
A4 | YEL/BLK | 625 | Vehicle Anti-Theft System - Starter Enable Relay Output - Coil
A5 | DK GRN | 264 | Security Indicator Lamp Feed
A6-A8 | -- | -- | Not Used
B1 | -- | -- | Not Used
B2 | PNK | 139 | Fused Output - IGN
B3-B4 | -- | -- | Not Used
B5 | BLK/WHT | 251 | Ground
B6 | BLK/WHT | 251 | Ground
B7 | PPL/WHT | 1074 | Ignition Key Resistor Return
B8 | WHT/BLK | 1073 | Ignition Key Resistor Feed

#### Rear Compartment Lid Tamper Switch

Connector Part Information |

• | 08900863

• | 2-Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 263 | Tamper Switch Signal
B | BLK | 1250 | Ground