For 1990-2009 cars

1. Inspect the second clutch housing assembly (617) for the following:

• | A leaking or damaged ball check valve in the second clutch housing. Turn the housing in order to seat the check ball. Use transmission fluid in order to check for leaks.

• | Scored or worn bushings

• | Discolored band surface or wear on the drum caused by excess heat

• | Flatness of the band surface on the drum

• | Damaged reverse reaction drum splines

• | Cracks in welds

2. Inspect the backing plate (626) and the waved plate (623) of the second clutch for cracks or heat spots.
3. Inspect the steel plates (625) and the apply plate (716) of the second clutch for wear.
4. Inspect the fiber plates (624) of the second clutch for wear, flaking, or lining separation.
5. Inspect the spring assembly (621) of the second clutch for damage to the ring cage. Check for distorted or missing springs.
6. Inspect the spring snap ring (622) of the second clutch for damage. Inspect the snap ring (627) of the second clutch backing plate for damage.