For 1990-2009 cars

## Power Mirror Switch Replacement Pontiac

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the armrest applique.

Insert a small thin-bladed tool at the front of the applique in order to release the retaining clip.

3. Disconnect the electrical connector.
4. Loosen the setscrew that attaches the mirror control to the applique.
5. Remove the power mirror switch.

### Installation Procedure

1. Install the power mirror switch to the applique.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the setscrew.

Tighten
Tighten the setscrew to 0.4 N·m (4 lb in).

3. Connect the electrical connector.
4. Install the armrest applique.
5. Connect the negative battery cable.

## Power Mirror Switch Replacement Oldsmobile

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the trim panel retaining fasteners from the lower armrest bezel.
3. Remove the lower armrest bezel.

Use a thin-bladed tool.

4. Disengage the switch plate retainer clips.

Insert a small, flat-blade tool between the switch plate and the trim panel.

5. Lift the switch plate.
6. Disconnect the electrical connectors.
7. Remove the setscrew.
8. Remove the mirror switch.

### Installation Procedure

1. Install the mirror control switch to the switch plate.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the setscrew.

Tighten
Tighten the setscrew to 0.8 N·m (7 lb in).

3. Connect the electrical connectors.
4. Install the switch plate in the trim panel.

Push inward the switch plate.

5. Install the trim panel retaining fasteners.
6. Connect the negative battery cable.