For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Remote Keyless Entry System Check? | -- | Go to Step 2 | Go to Remote Keyless Entry System Check
2 |

1. Hold the transmitter within the range of the vehicle.
2. Press and hold the lock and unlock buttons on the transmitter for 8 seconds.

Did the locks cycle?

--

Go to Step 3

Go to Step 4

3 | Operate the lock and unlock functions from the transmitter. Does the transmitter work? | -- | Go to Step 6 | Go to Step 5
4 | Replace the transmitter. Refer to Transmitter Programming . Is the repair complete? | -- | Go to Step 6 | --
5 | Replace the RFA module. Refer to Remote Control Door Lock Receiver Replacement . Is the repair complete? | -- | Go to Step 6 | --
6 |

1. Ensure that any components removed during diagnosis are installed.
2. Ensure that all of the connectors are connected.

Is the repair complete?

--

Go to Remote Keyless Entry System Check

--