For 1990-2009 cars

### Removal Procedure

1. Remove horseshoe clip (1) from front of shift control knob, and remove knob.
2. Remove the console. Refer to Console Replacement in Instrument Panel, Gages and Console.
3. Remove the console wiring harness.
4. Remove the console shift control wiring harness.
5. Remove the automatic transaxle range selector cable. Refer to Range Selector Lever Cable Replacement .
6. Remove the park/lock cable. Refer to Park Lock Cable Replacement .
7. Remove the console shift control nuts.
8. Remove the console shift control.

### Installation Procedure

1. Install the console shift control.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the console shift control nuts.

Tighten
Tighten the console shift control nuts to 24 N·m (18 lb ft).

3. Install the park/lock cable. Refer to Park Lock Cable Replacement .
4. Install the automatic transaxle range selector cable. Refer to Range Selector Lever Cable Replacement .
5. Install the console shift control wiring harness.
6. Install the console wiring harness.
7. Install the console. Refer to Console Replacement in to Instrument Panel, Gages and Console.
8. Adjust the transaxle range selector cable. Refer to Range Selector Lever Cable Replacement and/or Range Selector Lever Cable Adjustment .