For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Inlet Grille Panel Screws | 1.9 N·m | 17 lb in
Center Brace to Radiator Support Bolts | 13 N·m | 115 lb in
Fender Sound Insulator Bolts | 1.7 N·m | 17 lb in
Fender to Body Bolts | 9.5 N·m | 84 lb in
Front End Panel to Body Bolts | 5 N·m | 44 lb in
Grille Bolts - Eighty Eight/LSS | 4 N·m | 35 lb in
Grille Bolts - Regency | 1.9 N·m | 17 lb in
Grille to Hood Bolts - Pontiac | 1.9 N·m | 17 lb in
Grille to Hood Nuts - Buick | 1.9 N·m | 17 lb in
Hood Hinges to Upper Rail Bolts | 29 N·m | 21 lb ft
Hood Latch Release Handle Bolts | 7 N·m | 62 lb in
Hood Panel to Hinge Bolts | 29 N·m | 21 lb ft
Lower Air Deflector Bolts | 7.5 N·m | 66 lb in
Primary Latch Bolts | 9.5 N·m | 84 lb in
Secondary Latch to Hood Bolts | 9.5 N·m | 84 lb in
Side Brace to Center Brace on Radiator Support Bolts | 9.5 N·m | 84 lb in
Wheel Opening Molding Screws - Buick | 1.9 N·m | 17 lb in
Wheel Opening Molding Screws - Eighty Eight/LSS | 2.1 N·m | 18 lb in
Wheelhouse Assembly Bolts | 1.9 N·m | 17 lb in