For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.

Important: Before disconnecting the air hose from the intake air filter or the air compressor, clean the components and the surrounding area to prevent dirt and other foreign material from entering the air compressor.

2. Disconnect the intake air filter from the body rail and the air hose.

### Installation Procedure

1. Connect the intake air filter to the air hose and the body rail.
2. Lower the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.