For 1990-2009 cars

• | The front seat belt retractor is attached to the rocker with a bolt.

• | The front seat belt guide loop is attached to the upper center pillar with a bolt.

• | The buckle end of the front seat belt is attached to the load bar assembly attached to the floor pan with a bolt.

• | The center occupant belt is attached to the floor pan on the seat rail.

The driver's seat belt system includes a seat belt switch in the driver seat buckle-side belt which controls a reminder lamp and a tone alarm.

In order to diagnose a failure of the reminder lamp or tone alarm, refer to Audible Warnings System Check in Instrument Panel, Gauges and Console.

The rear belt system includes the following components:

• | The rear center belt buckle is attached to the floor pan with a nut.

• | The latch is on the right and the buckle is on the left.

• | The rear seat shoulder belt retractor is attached to the rear window panel with a bolt.

| The rear seat outer belt anchor is attached to the floor pan with a bolt.