For 1990-2009 cars

#### Removal Procedure

1. Move the driver's seat forward.
2. Cut the carpet back under the driver's seat to expose the control module.
3. Disconnect the electrical connector from the control module.
4. Remove the two screws and the control module.

#### Installation Procedure

1. Install the control module with two screws.
2. Connect the electrical connector to the module.
3. Install the carpet.