For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 37096 Flywheel Holding Tool

• | J 38197-A Crankshaft Balancer Puller

• | J 36660-A Torque Angle Meter

1. Hold the flywheel. Use the J 37096 .
2. Remove the balancer bolt.

Important: Do not attempt to separate the pulley from the balancer hub. The balancer is serviced as an assembly.

3. Use the J 38197-A in order to remove the crankshaft balancer. Use 1/4 in bolts to attach to the pulley. Screw them in 1/4 in.

### Installation Procedure

#### Tools Required

• | J 37096 Flywheel Holding Tool

• | J 36660-A Torque Angle Meter

1. Lubricate the seal surface with engine oil.
2. Install the crankshaft balancer.

Notice: This bolt is designed to permanently stretch when tightened, and therefore MUST be replaced anytime it is removed. The correct part number fastener must be used to replace this type of fastener. Do not use a bolt that is stronger in this application. If the correct bolt is not used, the parts will not be tightened correctly. The system or the components may be damaged.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the balancer bolt. Hold the flywheel with the J 37096 .

Tighten
Tighten the bolt to 150 N·m (111 lb ft). Use the J 36660-A in order to rotate the bolt an additional 76 degrees.