For 1990-2009 cars

### Removal Procedure

1. Remove the Intake Air Temperature (IAT) sensor electrical connector (1) from the IAT sensor (2).
2. Remove the air intake duct from the throttle body.
3. Remove the snap ring (3) from the throttle body (1).
4. Remove the throttle body air inlet screen (2) from the throttle body (1).

### Installation Procedure

1. Install the throttle body air inlet screen (2) into the throttle body (1).
2. Install the snap ring on to the throttle body.
3. Install the air intake tube.

Tighten
Tighten the air intake tube clamp to 2 N·m (18 lb in).

4. Install the IAT sensor electrical connector (1) to the IAT sensor (2).