For 1990-2009 cars

### Removal Procedure

1. Refer to Seat Replacement in order to remove the following components:

• | The seat

• | The adjusters

2. Remove the seat back (2) from the seat.
3. Remove the recliner handle or the power recliner switch, if applicable.
4. Remove the armrest. Refer to Front Seat Armrest Replacement .
5. Remove the hog rings (1) and the cushion cover.
6. Remove the J-section retainer (5).
7. Remove the hog rings and the pad from the springs (3).
8. Remove the pad and the cover from the frame.
9. Remove the hog rings (2) and the cover from the bottom of the cushion.
10. Remove the hog rings in the pad behind the cover.
11. Disengage the hook and loop strips (2).

### Installation Procedure

1. Align the locating holes in the cover with the work lines on the pad.
2. Install the hog rings in the pad behind the cover (1).
3. Install the hog rings (2) and the cover to the bottom of the cushion.
4. Install the pad and the cover to the frame.
5. Install the hog rings and the pad to the springs (3).
6. Install the J-section retainer (5).
7. Install the hog rings (1) and the cushion cover.
8. Install the armrest. Refer to Front Seat Armrest Replacement .
9. Install the recliner handle or the power recliner switch, if applicable.
10. Install the seatback (2) to the seat.
11. Refer to Seat Replacement in order to install the following components:

• | The seat

• | The adjusters