For 1990-2009 cars

### Removal Procedure

1. Remove the windshield defroster grille. Refer to Defroster Grille Replacement
2. Remove the screws (1) from the HUD module (2) to IP.
3. Lift the HUD module (2) from the IP.
4. Disconnect the electrical connector (3).

### Installation Procedure

1. Connect the electrical connector (3).
2. Install the lower HUD module (2) into the IP.
3. Install the screws (1) retaining the HUD module to the IP.
4. Install the windshield defroster grille. Refer to Defroster Grille Replacement .